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SD1 - NRA Self-Declaration Form – End of Queue 
Note: Upon completing this document, please ensure to sign it by double-clicking in the designated signature area located at the end of the document.
	Original submission date (DD/MM/YYYY):
	04/05/2026
	Last updated
(DD/MM/YYYY):
	11/05/2026

	Document reference:
	Provided by DFRS

	Company name:
	NRA XYZ

	Country:
	Country XYZ

	Data Version Information 
(e.g. v2.x, v3.x, etc.):
	v1

	Data Format:
	Data is shared in the format:
☐ JSON
☒  XML

	Data Processing Level:
	☐ L2
☒ L3

	Location Preference:
	☒ OpenLR  
☐  Alert-C
☐  GML
☐  TPEG

	Information available from NRA road system:
	☒ all sections of the road network as designated by the Member State
☐ the road network as described in the appendix: ______________________________

	Access point or data provision:
	☒ National accesspoint – URL for access instructions: 
	www.instructions.com

	
	☒ MDS
	Connector Description

	
	☐ Other: Further description

	

	Conditions of use:
	Free to use/list conditions here



Description of data elements provided 
	
	Data element name
	Provided
	Example
	Further details example

	Minimal data set
	Submitter
	☐
	NRA XYZ
	Company Reference ID

	
	Location reference
	☐
	Area, Linear, Point
	

	
	Location coordinates
	☐
	51.47961920,7.27943700 
	WGS84 Decimal Lat Lon 

	
	Timestamp
	☐
	1722513751011
	UTC timezone

	
	Direction
	☐
	347
	Degrees heading

	
	Type according to submitter original use case
	☐
	SLIPPERY_ROAD
	

	Optional Data or Extensions (add as many as you have)
	Event-ID
	☐
	d4190f3e-e027-4282
	UUID

	
	Trace
	☐
	
	Number of trace points

	
	ProbabilityOfOccurance
	☐
	certain , improbable , probable , risk of
	

	
	SupplierObservationConfidence
	☐
	86
	Indicates the confidencelevel of the supplier on a scale from 0 to 100.
XMI file or link for more detailed SituationRecordExtension information

	
	Information about end of situation 
	☐
	Cancellation: true
	Indicates if event has information about it’s end

	
	Timeliness 
	☐
	10 Minutes internal NRA processing time 
	

	
	Update cycle
	☐
	Every 10 sec
	

	
	Validity duration
	☐
	30 Minutes
	

	
	Functional Road Classes
	☐
	FRC2, rural road
	

	
	Location Accuracy
	☐
	<10m
	

	
	Data sources
	☐
	Road-surface-condition-sensor X2, 
weather station SOL2, 
Police, 
Traffic Center manual information,
Road service vehicle

	Add existing and real contributing data sources


	
	Data source information
	☐
	Weather stations: 
Station information: station.info.com

Sensor data information:
www.sensor.info.com

Police/Traffic Center manual information: 
Direct call from patrol to the on-duty police officer at the Traffic Control Centre

	Information/links to mentioned sources above and some detail to their functionality.





Contact point for technical enquiries 
It is essential that these contact details are actively monitored and that responses to enquiries are provided in a timely manner.
	Company name:
	NRA XYZ

	Company unit/division/section/team:
	Section XYZ

	Contact person name:
	

	Contact email address:
	

	Contact phone number:
	

	National Access Point:
	www.yournationalaccesspoint.com 



Signed (when completed)
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